{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":20,"n_cols":8,"rows_kept":20,"merged":[[1,0,1,7],[19,0,19,3]],"flags":["formulas_cached_only"]}
[]
["The spreadsheet is based on the calculations done here : http://interface.khm.de/index.php/lab/experiments/sleep_watchdog_battery/"]
[]
["Capacity of AA (mAh)",2500]
[]
["Device","Power on (mA)","power in sleep (mA)","Time on (ms)","Time in sleep (ms)","Approx battery life hours","Approx battery life days","Approx battery life months"]
["Mobile monitor, 1 CT channel and old RF",13,0.03,332,4000,"","",""]
["emonTx V1.4, two CT channels RF12, using sleepy and RFsleep",14,0.1,332,4000,"","",""]
{"$rows_empty":11}
["By Glyn Hudson openenergymonitor.org/emon/emontx"]