<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>FTDI</text>
<text>BLK</text>
<text>REG</text>
<text>GRN</text>
<text>ANT</text>
<hole x="3.175" y="3.175" drill="3.2"/>
<hole x="46.355" y="3.175" drill="3.2"/>
<hole x="3.175" y="46.355" drill="3.2"/>
<wire x1="46.355" y1="0" x2="3.175" y2="0" width="0.0254" layer="20"/>
<wire x1="0" y1="3.175" x2="0" y2="46.355" width="0.0254" layer="20"/>
<wire x1="3.175" y1="49.53" x2="46.355" y2="49.53" width="0.0254" layer="20"/>
<text>RH005.1
Oct 2014</text>
<text>LED Node
Richard Hawthorn
richardhawthorn.com</text>
<text>Charging</text>
<hole x="46.355" y="46.355" drill="3.2"/>
<wire x1="49.53" y1="46.355" x2="49.53" y2="3.175" width="0.0254" layer="20"/>
<wire x1="3.175" y1="0" x2="0" y2="3.175" width="0.0254" layer="20" curve="-90"/>
<wire x1="49.53" y1="3.175" x2="46.355" y2="0" width="0.0254" layer="20" curve="-90"/>
<wire x1="46.355" y1="49.53" x2="49.53" y2="46.355" width="0.0254" layer="20" curve="-90"/>
<wire x1="0" y1="46.355" x2="3.175" y2="49.53" width="0.0254" layer="20" curve="-90"/>
<text>LED
GND</text>
<text>LED
VIN</text>
<text>LED
3.3v</text>
<text>LED
OUT</text>
<text>LED
OUT</text>
<text>LED
OUT</text>
<text>LED
IN</text>
<text>LED
IN</text>
<text>or</text>
<text>Short LED OUT for outside 4 LEDs only</text>
<text>Short LED IN for inside 4 LEDs only</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="RESONATOR-SMD">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="0603-CAP">
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="0805-CAP">
</package>
<package name="0603-LED">
</package>
<package name="RFM12B-ANTENNA">
</package>
<package name="RFM69W-MINPADS">
</package>
<package name="RFM12B-MINPADS">
</package>
<package name="USB-MINIB">
<description>Surface Mount USB Mini-B Connector</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="WS2812B">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="EIA7343">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="switch-tact">
<description>&lt;b&gt;Diptronics THMD &amp; SMD tact switches&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;DTS-3: 3.5x6mm THMD tact switch
&lt;li&gt;DTS-6, DTS-64: 6x6mm THMD tact switch
&lt;li&gt;DTSM-3: 3.5x6mm SMD tact switch
&lt;li&gt;DTSM-6, DTSM-64: 6x6mm SMD tact switch
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DTSM-3">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="X1" library="SparkFun" package="RESONATOR-SMD" value="16 MHz">
<attribute name="NAME"/>
</element>
<element name="U3" library="linear" package="SOT23" value="MCP1703CB">
<attribute name="NAME"/>
</element>
<element name="U1" library="LowPowerLab" package="TQFP32-08" value="ATMega-328">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="R1" library="LowPowerLab" package="0603-RES" value="10k">
<attribute name="NAME"/>
</element>
<element name="C1" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C4" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C2" library="LowPowerLab" package="0603-CAP" value="1u">
<attribute name="NAME"/>
</element>
<element name="C3" library="LowPowerLab" package="0805-CAP" value="10u">
<attribute name="NAME"/>
</element>
<element name="LED2" library="LowPowerLab" package="0603-LED" value="LED0603">
<attribute name="NAME"/>
</element>
<element name="R2" library="LowPowerLab" package="0603-RES" value="1k5">
<attribute name="NAME"/>
</element>
<element name="U$3" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value=""/>
<element name="U$1" library="LowPowerLab" package="RFM12B-ANTENNA" value="RFM12B_ANTENNA"/>
<element name="RF2" library="LowPowerLab" package="RFM69W-MINPADS" value="RFM69"/>
<element name="RF1" library="LowPowerLab" package="RFM12B-MINPADS" value="RFM12B"/>
<element name="U2" library="SparkFun" package="SOT23-5" value="MCP73831">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun" package="0603-CAP" value="4u7">
<attribute name="NAME"/>
</element>
<element name="R3" library="LowPowerLab" package="0603-RES" value="1k5">
<attribute name="NAME"/>
</element>
<element name="R4" library="LowPowerLab" package="0603-RES" value="2K">
<attribute name="NAME"/>
</element>
<element name="CN3" library="adafruit" package="JST-PH-2-SMT-RA" value="BATT">
<attribute name="VALUE"/>
</element>
<element name="CN1" library="LowPowerLab" package="USB-MINIB" value="USB">
<attribute name="VALUE"/>
</element>
<element name="LED1" library="LowPowerLab" package="0603-LED" value="LED0603">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="1 uF">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="100 K">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="SCHOTTKY">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MOSFET">
<attribute name="NAME"/>
</element>
<element name="CN4" library="pinhead" package="1X06" value="FTDI"/>
<element name="L1" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L2" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L3" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L4" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L5" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L6" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L7" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L8" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L9" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L10" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L11" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L12" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L13" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L14" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L15" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="L16" library="adafruit" package="WS2812B" value="WS2812B"/>
<element name="C8" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C9" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C10" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C11" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C12" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C13" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C14" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C15" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C16" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C17" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C18" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C19" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C20" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C21" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C22" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="C23" library="LowPowerLab" package="0603-CAP" value="0.1">
<attribute name="NAME"/>
</element>
<element name="ICSP1" library="pinhead" package="2X03" value="ICSP">
<attribute name="VALUE"/>
</element>
<element name="S1" library="switch-tact" package="DTSM-3" value="DTSM-3">
<attribute name="NAME"/>
</element>
<element name="S2" library="switch-tact" package="DTSM-3" value="DTSM-3">
<attribute name="NAME"/>
</element>
<element name="R6" library="LowPowerLab" package="0603-RES" value="100r">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ3" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="SJ2" library="SparkFun-Retired" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
</element>
<element name="C24" library="SparkFun-Capacitors" package="EIA7343" value="100uF">
<attribute name="PROD_ID" value="CAP-07890"/>
<attribute name="NAME"/>
</element>
<element name="U5" library="burr-brown" package="SOT223" value="REG1117">
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="MPN" value="REG1117"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="NAME"/>
</element>
<element name="SJ4" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
</element>
<element name="SJ5" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
</element>
<element name="SJ6" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
</element>
<element name="SJ7" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
</element>
<element name="SJ8" library="SparkFun-Passives" package="PAD-JUMPER-2-NO_YES_SILK" value="JUMPER-PAD-2-NOYES_SILK">
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun" package="SOT23-3" value="BSS138">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Passives" package="0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R9" library="LowPowerLab" package="0603-RES" value="100r">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="LED2" pad="MINUS"/>
<contactref element="RF2" pad="GND"/>
<contactref element="RF2" pad="GND"/>
<contactref element="RF1" pad="GND"/>
<contactref element="CN1" pad="GND"/>
<contactref element="C6" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="CN3" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="CN4" pad="1"/>
<contactref element="ICSP1" pad="6"/>
<contactref element="S2" pad="2"/>
<contactref element="S1" pad="2"/>
<contactref element="SJ3" pad="1"/>
<contactref element="U5" pad="1"/>
</signal>
<signal name="D10_SS">
<contactref element="U1" pad="14"/>
<contactref element="RF2" pad="NSS"/>
<contactref element="RF1" pad="SEL"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="ICSP1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$21">
<contactref element="X1" pad="3"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="20"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="PWR">
<contactref element="U3" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="CN4" pad="3"/>
<contactref element="SJ2" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="C1" pad="2"/>
<contactref element="CN4" pad="6"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="RF2" pad="VDD"/>
<contactref element="RF2" pad="VDD"/>
<contactref element="RF1" pad="VDD"/>
<contactref element="U3" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="ICSP1" pad="2"/>
<contactref element="SJ1" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="12"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="D1_TX">
<contactref element="U1" pad="31"/>
<contactref element="CN4" pad="5"/>
</signal>
<signal name="D0_RX">
<contactref element="U1" pad="30"/>
<contactref element="CN4" pad="4"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="A4_SDA">
<contactref element="U1" pad="27"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="26"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="24"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="23"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="RF2" pad="DIO0"/>
<contactref element="RF1" pad="IRQ"/>
</signal>
<signal name="D11_MOSI">
<contactref element="U1" pad="15"/>
<contactref element="RF2" pad="MOSI"/>
<contactref element="RF1" pad="SDI"/>
<contactref element="ICSP1" pad="4"/>
</signal>
<signal name="D12_MISO">
<contactref element="U1" pad="16"/>
<contactref element="RF2" pad="MISO"/>
<contactref element="RF1" pad="SDO"/>
<contactref element="ICSP1" pad="1"/>
</signal>
<signal name="D13_SCK">
<contactref element="U1" pad="17"/>
<contactref element="RF2" pad="SCK"/>
<contactref element="RF1" pad="SCK"/>
<contactref element="ICSP1" pad="3"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="A5_SCL">
<contactref element="U1" pad="28"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="Q2" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="PLUS"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$1"/>
<contactref element="RF2" pad="ANA"/>
<contactref element="RF1" pad="ANT"/>
</signal>
<signal name="VBAT">
<contactref element="U2" pad="3"/>
<contactref element="CN3" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="PLUS"/>
</signal>
<signal name="PROG">
<contactref element="U2" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="STAT">
<contactref element="U2" pad="1"/>
<contactref element="LED1" pad="MINUS"/>
</signal>
<signal name="VBUS">
<contactref element="CN1" pad="VBUS"/>
<contactref element="R3" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="D1" pad="A"/>
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="L2" pad="2-DOUT"/>
<contactref element="L3" pad="4-DIN"/>
</signal>
<signal name="LED-OUT-1">
<contactref element="L1" pad="2-DOUT"/>
<contactref element="L2" pad="4-DIN"/>
<contactref element="SJ6" pad="1"/>
</signal>
<signal name="LED-MID-1">
<contactref element="L5" pad="2-DOUT"/>
<contactref element="L6" pad="4-DIN"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="L6" pad="2-DOUT"/>
<contactref element="L7" pad="4-DIN"/>
</signal>
<signal name="LED-MID-2">
<contactref element="L7" pad="2-DOUT"/>
<contactref element="L8" pad="4-DIN"/>
<contactref element="SJ5" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="L8" pad="2-DOUT"/>
<contactref element="L9" pad="4-DIN"/>
</signal>
<signal name="LED-MID-3">
<contactref element="L9" pad="2-DOUT"/>
<contactref element="L10" pad="4-DIN"/>
<contactref element="SJ5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="L10" pad="2-DOUT"/>
<contactref element="L11" pad="4-DIN"/>
</signal>
<signal name="N$15">
<contactref element="L11" pad="2-DOUT"/>
<contactref element="L12" pad="4-DIN"/>
</signal>
<signal name="LED-OUT-2">
<contactref element="L3" pad="2-DOUT"/>
<contactref element="L4" pad="4-DIN"/>
<contactref element="SJ6" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="L14" pad="2-DOUT"/>
<contactref element="L15" pad="4-DIN"/>
</signal>
<signal name="LED-OUT-3">
<contactref element="L4" pad="2-DOUT"/>
<contactref element="L5" pad="4-DIN"/>
<contactref element="SJ7" pad="1"/>
</signal>
<signal name="LED_POS">
<contactref element="SJ1" pad="2"/>
<contactref element="L1" pad="1-VDD"/>
<contactref element="L2" pad="1-VDD"/>
<contactref element="L3" pad="1-VDD"/>
<contactref element="L4" pad="1-VDD"/>
<contactref element="L5" pad="1-VDD"/>
<contactref element="L6" pad="1-VDD"/>
<contactref element="L7" pad="1-VDD"/>
<contactref element="L8" pad="1-VDD"/>
<contactref element="C12" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="L13" pad="1-VDD"/>
<contactref element="L14" pad="1-VDD"/>
<contactref element="L15" pad="1-VDD"/>
<contactref element="L16" pad="1-VDD"/>
<contactref element="L9" pad="1-VDD"/>
<contactref element="L10" pad="1-VDD"/>
<contactref element="L11" pad="1-VDD"/>
<contactref element="L12" pad="1-VDD"/>
<contactref element="SJ2" pad="2"/>
<contactref element="C24" pad="A"/>
</signal>
<signal name="LED_NEG">
<contactref element="SJ3" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="L13" pad="3-GND"/>
<contactref element="L14" pad="3-GND"/>
<contactref element="L15" pad="3-GND"/>
<contactref element="L16" pad="3-GND"/>
<contactref element="L12" pad="3-GND"/>
<contactref element="L11" pad="3-GND"/>
<contactref element="L10" pad="3-GND"/>
<contactref element="L9" pad="3-GND"/>
<contactref element="L5" pad="3-GND"/>
<contactref element="L6" pad="3-GND"/>
<contactref element="L7" pad="3-GND"/>
<contactref element="L8" pad="3-GND"/>
<contactref element="L4" pad="3-GND"/>
<contactref element="L3" pad="3-GND"/>
<contactref element="L2" pad="3-GND"/>
<contactref element="L1" pad="3-GND"/>
<contactref element="C24" pad="C"/>
</signal>
<signal name="LED_DATA">
<contactref element="R6" pad="2"/>
<contactref element="L1" pad="4-DIN"/>
<contactref element="SJ4" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="LED-OUT-4">
<contactref element="L12" pad="2-DOUT"/>
<contactref element="L13" pad="4-DIN"/>
<contactref element="SJ7" pad="2"/>
</signal>
<signal name="LED-OUT-5">
<contactref element="L13" pad="2-DOUT"/>
<contactref element="L14" pad="4-DIN"/>
<contactref element="SJ8" pad="1"/>
</signal>
<signal name="LED-OUT-6">
<contactref element="L16" pad="4-DIN"/>
<contactref element="L15" pad="2-DOUT"/>
<contactref element="SJ8" pad="2"/>
</signal>
<signal name="HV_LED">
<contactref element="Q2" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
