{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Material"],"not_rendered":{"external_links":1,"defined_names":5},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Material","index":0,"n_rows":119,"n_cols":12,"rows_kept":119,"flags":["formulas_cached_only"]}
[null,"Material List for PLUTO-L16-2 circuit board"]
[{"$nulls":7},"D","= www.digikey.com",null,null,"12/30/08  DR-SL"]
[{"$nulls":3}," ",{"$nulls":3},"M","= www.mouser.com"]
[null,"Quantity",{"$nulls":8}," "]
[null,"per","per",{"$nulls":7},"Order","Where used &"]
[null,"order ","pcb","Value",null,"Attributes","Mfct-Series",null,"Part No.","$ each","$ total","designation on PCB"]
[]
[null,10,1,"LED",null,"LED, green","Lumex","D","67-1098-ND",{"v":0.103,"d":"$0.10"},{"v":1.03,"d":"$1.03"},"D2, long lead = (+)"]
[null,2,1," 2KBP01M-E4/51",null,"Bridge rectifier","Gen. Semicond.","D","2KBP01M-E4/51GI-ND",{"v":0.69,"d":"$0.69"},{"v":1.38,"d":"$1.38"},"D 1"]
[null,2,1,"L78M15ABV",null,"+15V regulator","STMicroelectronics","D","497-1465-5-ND",{"v":0.86,"d":"$0.86"},{"v":1.72,"d":"$1.72"},"Pos"]
[null,2,1,"LM79M15CT-ND",null,"-15V regulator","NS","D","LM79M15CT-ND",{"v":1.84,"d":"$1.84"},{"v":3.68,"d":"$3.68"},"Neg"]
[null,2,1,"85VDC",null,"Trnasient/Surge Absorber","Panasonic","D","P7240-ND",{"v":0.25,"d":"$0.25"},{"v":0.5,"d":"$0.50"},"SR1"]
[null,5,1,"1.0A SB",null,"3AG Fuse","Littelfuse","D","F2543-ND",{"v":0.934,"d":"$0.93"},{"v":4.67,"d":"$4.67"},"F1 (115VAC)"]
[null,0,1,"0.5A SB",null,"3AG Fuse","Littelfuse","D","F2538-ND",{"v":0.934,"d":"$0.93"},{"v":0,"d":"$0.00"},"F1 (230VAC)"]
[null,10,2,"clips",null,"fuse clips","Littelfuse","D","F040-ND",{"v":0.225,"d":"$0.23"},{"v":2.25,"d":"$2.25"},"F1"]
[]
[null,12,6,"OPA2134",null,"opamp","Burr-Brown/TI","D","OPA2134PA-ND",{"v":2.43,"d":"$2.43"},{"v":29.160000000000004,"d":"$29.16"},"U 1, 2, 3, 4, 5, 6"]
[null,12,6,"8-pin, tin",null,"IC sockets","Assmann","D","AE9986-ND",{"v":0.263,"d":"$0.26"},{"v":3.156,"d":"$3.16"},"U 1, 2, 3, 4, 5, 6"]
[null,6,3,"LM3886T",null,"IC power amp","NS","D","LM3886T-ND",{"v":7.14,"d":"$7.14"},{"v":42.839999999999996,"d":"$42.84"},"U 7, 8, 9"]
[null,0,3,"TO220",null,"heat sink, 4C/W","IERC","D","294-1082-ND",{"v":3.95,"d":"$3.95"},{"v":0,"d":"$0.00"},"(alternative component)"]
[null,6,3,"TO220",null,"heat sink, 4C/W","IERC","D","294-1086-ND",{"v":4.34,"d":"$4.34"},{"v":26.04,"d":"$26.04"},"(screwed onto U 7, 8, 9)"]
[null,1,1,"Silicone Base",null,"Heat Sink Grease","ITW Chemtronics","D","CT40-5-ND",{"v":20.15,"d":"$20.15"},{"v":20.15,"d":"$20.15"},"(between heat sink and IC U 7, 8, 9)"]
[]
[null,2,1,"phono jack",null,"RCA input, gold plated","Kobiconn","M","161-4217",{"v":1.08,"d":"$1.08"},{"v":2.16,"d":"$2.16"},"J1"]
[null,0,1,"phono jack",null,"RCA input, tin plated","CUI Stack","D","CP-1400-ND",{"v":0.66,"d":"$0.66"},{"v":0,"d":"$0.00"},"(alternative component)"]
[]
[null,0,1,"1k var",null,"trim pot","Bourns-3345P","D","3345P-102-ND",{"v":9.54,"d":"$9.54"},{"v":0,"d":"$0.00"},"VR1 "]
[null,2,1,"1k var",null,"trim pot","Bourns-3362P","D","3362P-1-102LF-ND",{"v":0.83,"d":"$0.83"},{"v":1.66,"d":"$1.66"},"VR1 (very small pointer alternative)"]
[]
[null,2,1,"50VA, 44VCT",null,"transformer, 22V@2.272A","Amveco","D","TE62085-ND",{"v":41.24,"d":"$41.24"},{"v":82.48,"d":"$82.48"},"(wired to) Primary & Secondary"]
[null,0,1,"50VA, 44VCT",null,"transformer, 22V@2.272A","Amveco","D","TE70085-ND",{"v":43.36,"d":"$43.36"},{"v":0,"d":"$0.00"},"(alternative component)"]
[{"$nulls":10}," "]
[null,2,1,"110V power cord",null,"2 cond., 9ft","Assmann","D","AE9903-ND",{"v":7.85,"d":"$7.85"},{"v":15.7,"d":"$15.70"},"(wired to) 110VAC"]
[null,1,"1/2","Audio cable",null,"2RCA male to male, 16ft","Assmann","D","AE1407-ND",{"v":9.64,"d":"$9.64"},{"v":9.64,"d":"$9.64"},"(between J1 and preamp output)"]
[{"$nulls":10}," "]
[null,2,1,"Binding post",null,"red","Johnson","D","111-0102-001",{"v":2.4,"d":"$2.40"},{"v":4.8,"d":"$4.80"},"(wired to) J2+"]
[null,2,1,"Binding post",null,"black","Johnson","D","111-0103-001",{"v":2.4,"d":"$2.40"},{"v":4.8,"d":"$4.80"},"(wired to) J2-"]
[{"$nulls":10}," "]
[null,8,4,"0.25\" tall (4-40)",null,"Hex threaded standoff","Keystone","D","8714K-ND",{"v":0.377,"d":"$0.38"},{"v":3.016,"d":"$3.02"},"(for pcb mounting)"]
[null,14,7,"4-40",null,"flat head screw, 0.5inch",{"$nulls":4}," ","(for U 7, 8, 9 7 & pcb mounting)"]
[null,14,7,"4-40",null,"hex nut",{"$nulls":4}," ","(for U 7, 8, 9 7 & pcb mounting)"]
[null,1,"1/2","5 lugs",null,"Solder-type terminal strip","Radio Shack",null,"274-688",{"v":1.29,"d":"$1.29"},{"v":1.29,"d":"$1.29"},"(for tweeter wiring)"]
[]
[{"$nulls":10},{"v":260.832,"d":"$260.83"}]
[null,"Quantity"]
[null,"per","per",{"$nulls":7},"Order"]
[null,"order ","pcb","Value",null,"Attributes","Mfct-Series",null,"Part No.","$ each","$ total","Designation on PCB"]
[{"$nulls":10}," "]
[null,5,2,"jumper",null,"Zerohm Jumper Wire","YAGEO-MFR","D","0.0QBK-ND",{"v":0.06,"d":"$0.06"},{"v":0.3,"d":"$0.30"},"R 66,  C3"]
[null,null,2,"jumper",null,"Zerohm Jumper Wire","YAGEO-MFR","D","0.0QBK-ND",{"v":0.06,"d":"$0.06"},{"v":0,"d":"$0.00"},"R101, 102 for 110VAC"]
[null,null,1,"jumper",null,"Zerohm Jumper Wire","YAGEO-MFR","D","0.0QBK-ND",{"v":0.06,"d":"$0.06"},{"v":0,"d":"$0.00"},"R103 for 220VAC"]
[]
[null,5,1,2.2,null,"metal oxyde, 5%, 1W","YAGEO-MFR","D","2.2W-1-ND",{"v":0.16,"d":"$0.16"},{"v":0.8,"d":"$0.80"},"R 108"]
[null,5,2,150,null,"metal oxyde, 5%, 1W","YAGEO-MFR","D","150W-1-ND",{"v":0.16,"d":"$0.16"},{"v":0.8,"d":"$0.80"},"R 106, 107"]
[null,5,1,"1.0k",null,"metal oxyde, 5%, 1W","YAGEO-MFR","D","1.0kW-1-ND",{"v":0.15,"d":"$0.15"},{"v":0.75,"d":"$0.75"},"R 4"]
[]
[null,5,1,100,null,"metal film, 1%, 1/4W","YAGEO-MFR","D","100XBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R 5"]
[null,5,2,511,null,"metal film, 1%, 1/4W","YAGEO-MFR","D","511XBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R 33, 63"]
[null,5,1,750,null,"metal film, 1%, 1/4W","YAGEO-MFR","D","750XBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R32"]
[null,5,1,"1.00k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","1.00kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R 1"]
[null,10,4,"1.96k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","1.96kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":1,"d":"$1.00"},"R 6, 43, 83, 93"]
[null,10,4,"2.61k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","2.61kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":1,"d":"$1.00"},"R 21, 31, 61, 62"]
[null,5,1,"2.87k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","2.87kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R289 at R28-R29 junction"]
[null,30,13,"3.48k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","3.48kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":3,"d":"$3.00"},"R 3, 23, 24, 26, 28, 29, 30, 51, "]
[{"$nulls":9}," ",null,"R 52, 53, 54, 68, 69"]
[null,10,4,"6.81k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","6.81kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":1,"d":"$1.00"},"R 25, 27, 104, 105"]
[null,5,2,"8.25k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","8.25kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R 55, 56"]
[null,5,2,"12.1k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","12.1kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R57, 60"]
[null,15,5,"21.5k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","21.5kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":1.5,"d":"$1.50"},"R 58, 59,42,82,92"]
[null,5,1,"31.6k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","31.6kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":0.5,"d":"$0.50"},"R 2"]
[null,10,3,"38.3k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","38.3kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":1,"d":"$1.00"},"R 41, 81, 91"]
[null,10,3,"100k",null,"metal film, 1%, 1/4W","YAGEO-MFR","D","100kXBK-ND",{"v":0.1,"d":"$0.10"},{"v":1,"d":"$1.00"},"R 34, 64, 65"]
[{"$nulls":9},"  "," "]
[null," ",2,null,null,"R  not loaded",{"$nulls":5},"R22,  R67 "]
[null,null,1,null,null,"R  not loaded",{"$nulls":5},"R103 for 110VAC"]
[null,null,2,null,null,"R  not loaded",{"$nulls":5},"R101, 102 for 220VAC"]
[]
[{"$nulls":10},{"v":16.15,"d":"$16.15"}]
[]
[]
[null,"Quantity"]
[null,"per","per","Label-",{"$nulls":6},"Order"]
[null,"order ","pcb","Value",null,"Attributes","Mfct-Series"," ","Part No.","$ each","$ total","Designation on PCB"]
[]
[null,12,6,"220pF",null,"polyester, 10%","Panas-ECQ-P","D","P3893-ND",{"v":0.194,"d":"$0.19"},{"v":2.3280000000000003,"d":"$2.33"},"C 2, 4, 21, 27, 63, 68 "]
[null,6,3,"820pF",null,"polyester, 10%","Panas-ECQ-P","D","P3900-ND",{"v":0.23,"d":"$0.23"},{"v":1.3800000000000001,"d":"$1.38"},"C41, 81, 91"]
[{"$nulls":10}," "]
[null,2,1,"2.2nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3222-ND",{"v":0.46,"d":"$0.46"},{"v":0.92,"d":"$0.92"},"C289 from R289 to ground"]
[null,2,1,"2.7nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3272-ND",{"v":0.46,"d":"$0.46"},{"v":0.92,"d":"$0.92"},"C 29"]
[null,2,1,"10nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3103-ND",{"v":0.53,"d":"$0.53"},{"v":1.06,"d":"$1.06"},"C 28, "]
[null,22,11,"33nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3333-ND",{"v":0.507,"d":"$0.51"},{"v":11.154,"d":"$11.15"},"C 22, 23, 24, 25, 51, 52, 53, 54, "]
[{"$nulls":5}," "," ",{"$nulls":4},"C 55, 56, 64"]
[{"$nulls":6}," "]
[null,4,2,"47nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3473-ND",{"v":0.64,"d":"$0.64"},{"v":2.56,"d":"$2.56"},"C 26, 65"]
[null,4,2,"100nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3104-ND",{"v":0.86,"d":"$0.86"},{"v":3.44,"d":"$3.44"},"C59, 62"]
[null,2,1,"150nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3154-ND",{"v":1.06,"d":"$1.06"},{"v":2.12,"d":"$2.12"},"C 66"]
[null,8,4,"330nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3334-ND",{"v":1.58,"d":"$1.58"},{"v":12.64,"d":"$12.64"},"C 1, 107, 108, 61"]
[null,2,1,"390nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3394-ND",{"v":1.89,"d":"$1.89"},{"v":3.78,"d":"$3.78"},"C58"]
[null,2,1,"470nF",null,"polypropylene, 2%","Panas-ECQ-P","D","P3474-ND",{"v":1.89,"d":"$1.89"},{"v":3.78,"d":"$3.78"},"C57"]
[]
[null,20,10,".01uF",null,"metal film","Panas-V","D","P4513-ND",{"v":0.1,"d":"$0.10"},{"v":2,"d":"$2.00"},"C 30, 31, 32, 33, 34, 35, 71, "]
[{"$nulls":11},"C 72, 75, 76, "]
[null,20,10,"0.1uF",null,"polyester, 450VDC","Panas-ECQE(C)","D","P10755-ND",{"v":0.528,"d":"$0.53"},{"v":10.56,"d":"$10.56"},"C  44, 45, 84, 85, 94, 95, 101,"]
[{"$nulls":11}," C 102, 109, 110,"]
[{"$nulls":10}," "]
[null,2,1,"1uF",null,"polyester","Panas-ECQ-E(F)","D","EF1105-ND",{"v":0.99,"d":"$0.99"},{"v":1.98,"d":"$1.98"},"C 43"]
[null,4,2,"10uF",null,"polyester","Panas-ECQ-E(F)","D","EF1106-ND",{"v":4.58,"d":"$4.58"},{"v":18.32,"d":"$18.32"},"C 83, 93"]
[]
[null,4,2,"33uF",null,"electrolytic,35V","Panas-FC","D","P10290-ND",{"v":0.34,"d":"$0.34"},{"v":1.36,"d":"$1.36"},"C 111, 112"]
[null,4,2,"470uF",null,"electrolytic, 50V","Panas-FC","D","P10328-ND",{"v":1.08,"d":"$1.08"},{"v":4.32,"d":"$4.32"},"C 105, 106"]
[]
[null,4,2,"22000uF",null,"electrolytic, 50V","Panas-TS","D","P6946-ND",{"v":8.21,"d":"$8.21"},{"v":32.84,"d":"$32.84"},"C 103, 104"]
[]
[null," ",5,null,null,"C  not loaded",{"$nulls":5},"C67, C42, C82, C92, C60"]
[{"$nulls":11}," "]
[]
[{"$nulls":10},{"v":117.46200000000002,"d":"$117.46"}]
[]
[{"$nulls":9},"total",{"v":394.444,"d":"$394.44"}]