{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":44,"n_cols":14,"rows_kept":44,"flags":["formulas_cached_only"]}
[]
[null,"SPL dependent driver behavior",{"$nulls":9},"LINKWITZ LAB    10/26/04"]
[]
[{"$nulls":4},"Driver A"]
[null,"Enter bold faced values",null,null,"Seas W22EX001",{"$nulls":3},"Piston Xpeak",null,"Piston force",null,"Kinetic energy"]
[{"$nulls":7},"Frequency","Monopole","Dipole","Monopole","Dipole","Monopole","Dipole"]
[{"$nulls":3},"SPL at 1m in free-space =",90,"dB",null,"Hz","mm","mm","N","N","mWs","mWs"]
[{"$nulls":7},20,{"v":27.26510717776763,"d":"27.3"},{"v":317.9656799071261,"d":"318.0"},{"v":6.071558909577459,"d":"6.1"},{"v":70.80652000349234,"d":"70.8"},{"v":58.36072883212614,"d":"58.36"},{"v":680.6028196402551,"d":"680.60"}]
[{"$nulls":3},"Piston area Sd =",220,"cm^2",null,{"v":28.284271247461902,"d":"28"},{"v":13.632553588883805,"d":"13.6"},{"v":112.41784422345992,"d":"112.4"},{"v":6.071558909577459,"d":"6.1"},{"v":50.06777044669035,"d":"50.1"},{"v":29.180364416063075,"d":"29.18"},{"v":240.62943453115457,"d":"240.63"}]
[{"$nulls":3},"Piston acceleration",{"v":30.945764065124663,"d":"30.9"},"x 9.81 m/s^2",null,{"v":40.00000000000001,"d":"40"},{"v":6.816276794441902,"d":"6.8"},{"v":39.74570998839072,"d":"39.7"},{"v":6.071558909577459,"d":"6.1"},{"v":35.40326000174616,"d":"35.4"},{"v":14.59018220803153,"d":"14.59"},{"v":85.07535245503185,"d":"85.08"}]
[{"$nulls":7},{"v":56.56854249492382,"d":"57"},{"v":3.408138397220951,"d":"3.4"},{"v":14.052230527932485,"d":"14.1"},{"v":6.071558909577459,"d":"6.1"},{"v":25.03388522334517,"d":"25.0"},{"v":7.295091104015762,"d":"7.30"},{"v":30.07867931639429,"d":"30.08"}]
[{"$nulls":3},"Moving mass Mms =",20,"g",null,{"v":80.00000000000003,"d":"80"},{"v":1.704069198610475,"d":"1.7"},{"v":4.9682137485488385,"d":"5.0"},{"v":6.071558909577459,"d":"6.1"},{"v":17.701630000873077,"d":"17.7"},{"v":3.6475455520078808,"d":"3.65"},{"v":10.634419056878974,"d":"10.63"}]
[{"$nulls":3},"Piston force",{"v":6.071558909577459,"d":"6.1"},"N",null,{"v":113.13708498984765,"d":"113"},{"v":0.8520345993052375,"d":"0.9"},{"v":1.7565288159915602,"d":"1.8"},{"v":6.071558909577459,"d":"6.1"},{"v":12.516942611672583,"d":"12.5"},{"v":1.8237727760039402,"d":"1.82"},{"v":3.759834914549285,"d":"3.76"}]
[{"$nulls":3},"Piston force",{"v":1.3644817595240046,"d":"1.4"},"lb",null,{"v":160.00000000000009,"d":"160"},{"v":0.42601729965261875,"d":"0.4"},{"v":0.6210267185686047,"d":"0.6"},{"v":6.071558909577459,"d":"6.1"},{"v":8.850815000436537,"d":"8.9"},{"v":0.91188638800197,"d":"0.91"},{"v":1.329302382109871,"d":"1.33"}]
[{"$nulls":6}," ",{"v":226.27416997969533,"d":"226"},{"v":0.21300864982630935,"d":"0.2"},{"v":0.21956610199894497,"d":"0.2"},{"v":6.071558909577459,"d":"6.1"},{"v":6.258471305836291,"d":"6.3"},{"v":0.45594319400098504,"d":"0.46"},{"v":0.46997936431866055,"d":"0.47"}]
[{"$nulls":3},"Dipole path difference D =",250,"mm",null,{"v":320.00000000000017,"d":"320"},{"v":0.10650432491315467,"d":"0.1"},{"v":0.07762833982107557,"d":"0.1"},{"v":6.071558909577459,"d":"6.1"},{"v":4.4254075002182685,"d":"4.4"},{"v":0.2279715970004925,"d":"0.23"},{"v":0.16616279776373388,"d":"0.17"}]
[{"$nulls":3},"Fequal",{"v":233.24,"d":"233"},"Hz",null,{"v":452.54833995939066,"d":"453"},{"v":0.05325216245657732,"d":"0.1"},{"v":0.027445762749868114,"d":"0.0"},{"v":6.071558909577459,"d":"6.1"},{"v":3.1292356529181453,"d":"3.1"},{"v":0.11398579850024626,"d":"0.11"},{"v":0.05874742053983257,"d":"0.06"}]
[{"$nulls":7},{"v":640.0000000000003,"d":"640"},{"v":0.02662608122828866,"d":"0.0"},{"v":0.01331304061414433,"d":"0.0"},{"v":6.071558909577459,"d":"6.1"},{"v":3.0357794547887296,"d":"3.0"},{"v":0.05699289925012312,"d":"0.06"},{"v":0.02849644962506156,"d":"0.03"}]
[{"$nulls":3},"Force factor Bl =",{"v":9,"d":"9.0"},"N/A",null,{"v":905.0966799187813,"d":"905"},{"v":0.013313040614144305,"d":"0.0"},{"v":0.006656520307072152,"d":"0.0"},{"v":6.071558909577459,"d":"6.1"},{"v":3.0357794547887296,"d":"3.0"},{"v":0.028496449625061565,"d":"0.03"},{"v":0.014248224812530783,"d":"0.01"}]
[{"$nulls":3},"Voice coil current",{"v":0.6746176566197177,"d":"0.67"},"A",null,{"v":1280.0000000000007,"d":"1280"},{"v":0.006656520307072141,"d":"0.0"},{"v":0.0033282601535360706,"d":"0.0"},{"v":6.071558909577459,"d":"6.1"},{"v":3.0357794547887296,"d":"3.0"},{"v":0.01424822481253078,"d":"0.01"},{"v":0.00712411240626539,"d":"0.01"}]
[{"$nulls":7},{"v":1810.1933598375626,"d":"1810"},{"v":0.00332826015353607,"d":"0.0"},{"v":0.001664130076768035,"d":"0.0"},{"v":6.071558909577459,"d":"6.1"},{"v":3.0357794547887296,"d":"3.0"},{"v":0.007124112406265391,"d":"0.01"},{"v":0.0035620562031326956,"d":"0.00"}]
[{"$nulls":3},"Voice coil resistance =",{"v":6,"d":"6.0"},"ohm",null,{"v":2560.0000000000014,"d":"2560"},{"v":0.0016641300767680466,"d":"0.0"},{"v":0.0008320650383840233,"d":"0.0"},{"v":6.071558909577459,"d":"6.1"},{"v":3.0357794547887296,"d":"3.0"},{"v":0.003562056203132695,"d":"0.00"},{"v":0.0017810281015663476,"d":"0.00"}]
[{"$nulls":3},"Power dissipation",{"v":2.730653895738476,"d":"2.7"},"W"]
[]
[]
[]
[]
[{"$nulls":4},"Driver B"]
[null,"Enter bold faced values",null,null,"Seas T25CF002",{"$nulls":3},"Piston Xpeak",null,"Piston force",null,"Kinetic energy"]
[{"$nulls":7},"Frequency","Monopole",null,"Monopole",null,"Monopole"]
[{"$nulls":3},"SPL at 1m in free-space =",90,"dB",null,"Hz","mm",null,"N",null,"mWs"]
[{"$nulls":7},500,{"v":1.371045389510602,"d":"1.37"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":1.706324786817494,"d":"1.71"}]
[{"$nulls":3},"Piston area Sd =",7,"cm^2",null,{"v":707.1067811865476,"d":"707"},{"v":0.6855226947553009,"d":"0.69"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.8531623934087467,"d":"0.85"}]
[{"$nulls":3},"Piston acceleration",{"v":972.5811563324894,"d":"972.6"},"x 9.81 m/s^2",null,{"v":1000.0000000000001,"d":"1000"},{"v":0.3427613473776496,"d":"0.34"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.42658119670437333,"d":"0.43"}]
[{"$nulls":7},{"v":1414.2135623730953,"d":"1414"},{"v":0.17138067368882476,"d":"0.17"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.21329059835218658,"d":"0.21"}]
[{"$nulls":3},"Moving mass Mms =",0.37,"g",null,{"v":2000.0000000000005,"d":"2000"},{"v":0.08569033684441237,"d":"0.09"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.10664529917609332,"d":"0.11"}]
[{"$nulls":3},"Piston force",{"v":3.5301778231400367,"d":"3.5"},"N",null,{"v":2828.427124746191,"d":"2828"},{"v":0.04284516842220618,"d":"0.04"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.053322649588046646,"d":"0.05"}]
[{"$nulls":3},"Piston force",{"v":0.7933486801803854,"d":"0.8"},"lb",null,{"v":4000.000000000002,"d":"4000"},{"v":0.021422584211103088,"d":"0.02"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.026661324794023313,"d":"0.03"}]
[{"$nulls":6}," ",{"v":5656.854249492383,"d":"5657"},{"v":0.010711292105551544,"d":"0.01"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.013330662397011656,"d":"0.01"}]
[{"$nulls":3},"Force factor Bl =",3.1,"N/A",null,{"v":8000.000000000005,"d":"8000"},{"v":0.005355646052775771,"d":"0.01"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.006665331198505828,"d":"0.01"}]
[{"$nulls":3},"Voice coil current",{"v":1.1387670397225924,"d":"1.14"},"A",null,{"v":11313.708498984768,"d":"11314"},{"v":0.0026778230263878855,"d":"0.00"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.0033326655992529123,"d":"0.00"}]
[{"$nulls":7},{"v":16000.000000000013,"d":"16000"},{"v":0.0013389115131939426,"d":"0.00"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.0016663327996264562,"d":"0.00"}]
[{"$nulls":3},"Voice coil resistance =",4.7,"ohm",null,{"v":22627.41699796954,"d":"22627"},{"v":0.0006694557565969712,"d":"0.00"},null,{"v":3.5301778231400367,"d":"3.5"},null,{"v":0.0008331663998132278,"d":"0.00"}]
[{"$nulls":3},"Power dissipation",{"v":6.094914742565216,"d":"6.1"},"W"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}