{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["phn-room2"],"not_rendered":{"images":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"phn-room2","index":0,"n_rows":72,"n_cols":16,"rows_kept":72,"flags":["formulas_cached_only"]}
["Room EQ with notch filters on PHOENIX pcb",{"$nulls":12},"12/16/09 SL"]
["Enter new numbers only in cells which are in BOLD print",{"$nulls":12},"3/24/00   LINKWITZ LAB"]
[]
[null,"Example filter",{"$nulls":3},"Filter 1",{"$nulls":3},"Filter 2",{"$nulls":3},"Filter 3"]
["Wanted","F0 =",20.2,"Hz",null,"F0 =",20.2,"Hz",null,"F0 =",38,"Hz",null,"F0 =",96,"Hz"]
[null,"dF =",2.5,"Hz",null,"dF =",2.5,"Hz",null,"dF =",3,"Hz",null,"dF =",5,"Hz"]
[null,"a =",-9,"dB =>",null,"a =",-9,"dB =>",null,"a =",-12,"dB =>",null,"a =",-3,"dB =>"]
[null,null,"a' =",{"v":0.3548133892335754,"d":"0.35"},null,null,"a' =",{"v":0.3548133892335754,"d":"0.35"},null,null,"a' =",{"v":0.251188643150958,"d":"0.25"},null,null,"a' =",{"v":0.7079457843841379,"d":"0.71"}]
[]
[null,"Synthesis",{"$nulls":3},"Synthesis",{"$nulls":3},"Synthesis",{"$nulls":3},"Synthesis"]
["Enter","R0 =",5110,"ohm",null,"R8 =",5110,"ohm",null,"R8 =",5110,"ohm",null,"R8 =",5110,"ohm"]
[null,"C3 =",{"v":0.000165,"d":"1.65E-04"},"F",null,"C13,14,15 =",{"v":0.000165,"d":"1.65E-04"},"F",null,"C16,17,18 =",{"v":0.000165,"d":"1.65E-04"},"F",null,"C21,22,23 =",{"v":0.00011,"d":"1.10E-04"},"F"]
[null,"R3 =",1,"ohm",null,"R3 =",1,"ohm",null,"R3 =",1,"ohm",null,"R3 =",0.5,"ohm"]
[null,"X3 =",{"v":47.751258053373945,"d":"48"},"j ohm",null,"X3 =",{"v":47.751258053373945,"d":"48"},"j ohm",null,"X3 =",{"v":25.38356349153036,"d":"25"},"j ohm",null,"X3 =",{"v":15.07149082309615,"d":"15"},"j ohm"]
[]
["Calculation","R =",{"v":2810.189158807515,"d":"2810"},"ohm",null,"R =",{"v":2810.189158807515,"d":"2810"},"ohm",null,"R =",{"v":1714.1486367175385,"d":"1714"},"ohm",null,"R =",{"v":12386.751379617699,"d":"12387"},"ohm"]
["#1","L =",{"v":178.9021982589885,"d":"179"},"H",null,"L =",{"v":178.9021982589885,"d":"179"},"H",null,"L =",{"v":90.93840957594327,"d":"91"},"H",null,"L =",{"v":394.2825421833022,"d":"394"},"H"]
[null,"C =",{"v":3.4699390579185684e-07,"d":"3.47E-07"},"F",null,"C =",{"v":3.4699390579185684e-07,"d":"3.47E-07"},"F",null,"C =",{"v":1.928971075320557e-07,"d":"1.93E-07"},"F",null,"C =",{"v":6.97092241495526e-09,"d":"6.97E-09"},"F"]
[null,"R1,2 =",{"v":1041.2760186541188,"d":"1041"},"ohm",null,"R13,14 =",{"v":1041.2760186541188,"d":"1041"},"ohm",null,"R17,18 =",{"v":742.3893023325686,"d":"742"},"ohm",null,"R19,20 =",{"v":1893.2476718910627,"d":"1893"},"ohm"]
[null,"R3' =",{"v":475.5126739861961,"d":"476"},"ohm",null,"R3' =",{"v":475.5126739861961,"d":"476"},"ohm",null,"R3' =",{"v":855.3783004370879,"d":"855"},"ohm",null,"R3' =",{"v":7889.91710508845,"d":"7890"},"ohm"]
[null,"R4 =",{"v":252.12444751308158,"d":"252"},"ohm",null,"R15 =",{"v":252.12444751308158,"d":"252"},"ohm",null,"R16 =",{"v":-626.0082683846867,"d":"-626"},"ohm",null,"R21 =",{"v":710.3389307471225,"d":"710"},"ohm"]
[]
[null,"Analysis",{"$nulls":3},"Analysis",{"$nulls":3},"Analysis",{"$nulls":3},"Analysis"]
["Select","R1 =",909,"ohm",null,"R13 =",1100,"ohm",null,"R17 =",681,"ohm",null,"R19 =",1780,"ohm"]
["based on","R2 =",1000,"ohm",null,"R14 =",1000,"ohm",null,"R18 =",619,"ohm",null,"R20 =",1620,"ohm"]
["calculation","R4 =",248,"ohm",null,"R15 =",10,"ohm",null,"R16 =",10,"ohm",null,"R21 =",10,"ohm"]
["#1","C =",{"v":3.9e-07,"d":"3.90E-07"},"F",null,"C12 =",{"v":3.9e-07,"d":"3.90E-07"},"F",null,"C19 =",{"v":2.7e-07,"d":"2.70E-07"},"F",null,"C20 =",{"v":1e-08,"d":"1.00E-08"},"F"]
[]
["Calculation","F0 =",{"v":20.80960872466297,"d":"20.8"},"Hz",null,"F0 =",{"v":18.91688019837584,"d":"18.9"},"Hz",null,"F0 =",{"v":36.7263185657347,"d":"36.7"},"Hz",null,"F0 =",{"v":89.36269970785233,"d":"89.4"},"Hz"]
["#2","dF =",{"v":2.7934620449842735,"d":"2.8"},"Hz",null,"dF =",{"v":2.267201776813483,"d":"2.3"},"Hz",null,"dF =",{"v":4.9548693424533035,"d":"5.0"},"Hz",null,"dF =",{"v":5.669799315891395,"d":"5.7"},"Hz"]
[null,"a =",{"v":-9.37022908416573,"d":"-9"},"dB",null,"a =",{"v":-9.473817735552215,"d":"-9"},"dB",null,"a =",{"v":-10.526436001431215,"d":"-11"},"dB",null,"a =",{"v":-3.240622593087346,"d":"-3"},"dB"]
[]
["Equivalent","R =",{"v":2.6325126739861964,"d":"2.63"},"k",null,"R =",{"v":2.585512673986196,"d":"2.59"},"k",null,"R =",{"v":2.165378300437088,"d":"2.17"},"k",null,"R =",{"v":11.29991710508845,"d":"11.30"},"k"]
["resonant","L =",{"v":149.985,"d":"150"},"H",null,"L =",{"v":181.5,"d":"182"},"H",null,"L =",{"v":69.553935,"d":"70"},"H",null,"L =",{"v":317.196,"d":"317"},"H"]
["circuit","C =",390,"nF",null,"C =",390,"nF",null,"C =",270,"nF",null,"C =",10,"nF"]
[null,"Q =",{"v":7.449397339057142,"d":"7.4"},null,null,"Q =",{"v":8.343712673409785,"d":"8.3"},null,null,"Q =",{"v":7.4121669064134,"d":"7.4"},null,null,"Q =",{"v":15.76117508381386,"d":"15.8"}]
[null,"T60 =",{"v":787.5532098065021,"d":"788"},"ms",null,"T60 =",{"v":970.3591548397893,"d":"970"},"ms",null,"T60 =",{"v":444.00767163533607,"d":"444"},"ms",null,"T60 =",{"v":388.020788290303,"d":"388"},"ms"]
{"$rows_empty":27}
["A corresponding spreadsheet could be designed for "]
["Inductor 2 as available on ORION (U10A)"]
["and THOR (U3A, U3B) printed circuits."]
["Each WM1 pcb has two Inductor 2 circuits."]
[]
[]
[]
["Notch filters from spreadsheet for obsolete Phoenix pcb:"]