<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>Switches, Keys...</description>
<packages>
<package name="SW8X8_SMD">
</package>
<package name="TL3315">
<description>E-Switch TL3315</description>
</package>
<package name="PTS840P">
<description>C&amp;K PTS840 PM SMTR LFS or PTS840 PK SMTR LFS</description>
</package>
<package name="GF1260159">
</package>
<package name="CUS22B">
<description>Copal Electronics CUS-22B</description>
</package>
<package name="TSWB3NCB111LFS">
</package>
<package name="SW6X6">
<description>Diptronics DTS6 or Omron B3F-10XX</description>
</package>
<package name="SW6X6_RIGHT">
<description>Diptronics DTSA6 or Omron B3F-31XX</description>
</package>
<package name="SW6X6_SMD">
<description>C&amp;K PTS645&lt;br&gt;
&lt;br&gt;
PTS645S-&lt;br&gt;
L - 130gr Black&lt;br&gt;
M - 160gr Blue&lt;br&gt;
H - 200gr Gray&lt;br&gt;
K - 260gr Red&lt;br&gt;
&lt;br&gt;
4.3-13mm height&lt;br&gt;</description>
</package>
<package name="DB3C">
<description>Cherry DB3C with PCB Terminals</description>
</package>
<package name="TL3305">
<description>E-Switch TL3305&lt;br&gt;
TL3305A - 3.8mm height&lt;br&gt;
TL3305B - 5.0mm height&lt;br&gt;
TL3305C - 7.0mm height&lt;br&gt;</description>
</package>
<package name="SW12X12">
<description>Diptronics DTS2</description>
</package>
<package name="MSS13PLP">
<description>Schukat MSS13PLP / Salecom TS-13P-A1-2-R1-E-H</description>
</package>
<package name="SKS06LP">
<description>Schukat SKS06LP / Salecom TS-6-TE1R1-E-H</description>
</package>
<package name="MSS13LSP">
<description>Schukat MSS13LSP / Salecom TS-13L-A1-2-R1-E-H</description>
</package>
<package name="PMC-1001THY">
</package>
</packages>
<symbols>
<symbol name="TACTILE-4">
<pin name="P1" direction="pas"/>
<pin name="S1" direction="pas"/>
</symbol>
<symbol name="SWITCH-2UM">
<pin name="C1" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="NO2" direction="pas"/>
<pin name="NC2" direction="pas"/>
</symbol>
<symbol name="TSWB3NCB111LFS">
<pin name="S1"/>
<pin name="A"/>
<pin name="B"/>
<pin name="S2"/>
<pin name="S3"/>
<pin name="S4"/>
<pin name="S5"/>
<pin name="COM_A"/>
<pin name="COM_B"/>
</symbol>
<symbol name="SWITCH-1UM">
<pin name="C1" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NC1" direction="pas"/>
</symbol>
<symbol name="SWITCH-1NC">
<pin name="C1" direction="pas"/>
<pin name="NC1" direction="pas"/>
</symbol>
<symbol name="SWITCH-1NO">
<pin name="C1" direction="pas"/>
<pin name="NC1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SW-TACTILE" prefix="SW">
<description>Tactile Switche</description>
<gates>
<gate name="SW" symbol="TACTILE-4"/>
</gates>
<devices>
<device name="-8X8_SMD" package="SW8X8_SMD">
<connects>
<connect gate="SW" pin="P1" pad="1 2"/>
<connect gate="SW" pin="S1" pad="3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TL3315" package="TL3315">
<connects>
<connect gate="SW" pin="P1" pad="1 4"/>
<connect gate="SW" pin="S1" pad="2 3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY" value="EG4621TR-ND"/>
</technology>
</technologies>
</device>
<device name="-PTS840P" package="PTS840P">
<connects>
<connect gate="SW" pin="P1" pad="1 2"/>
<connect gate="SW" pin="S1" pad="3 4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY" value="CKN10511DKR-ND"/>
</technology>
</technologies>
</device>
<device name="-6X6" package="SW6X6">
<connects>
<connect gate="SW" pin="P1" pad="1 2"/>
<connect gate="SW" pin="S1" pad="3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-6X6_SMD" package="SW6X6_SMD">
<connects>
<connect gate="SW" pin="P1" pad="1 2"/>
<connect gate="SW" pin="S1" pad="3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-6X6_RIGHT" package="SW6X6_RIGHT">
<connects>
<connect gate="SW" pin="P1" pad="1"/>
<connect gate="SW" pin="S1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TL3305" package="TL3305">
<connects>
<connect gate="SW" pin="P1" pad="1 4"/>
<connect gate="SW" pin="S1" pad="2 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-12X12" package="SW12X12">
<connects>
<connect gate="SW" pin="P1" pad="1 2"/>
<connect gate="SW" pin="S1" pad="3 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW-2UM" prefix="SW">
<description>Switch</description>
<gates>
<gate name="SW" symbol="SWITCH-2UM"/>
</gates>
<devices>
<device name="-CUS22B" package="CUS22B">
<connects>
<connect gate="SW" pin="C1" pad="2"/>
<connect gate="SW" pin="C2" pad="5"/>
<connect gate="SW" pin="NC1" pad="3"/>
<connect gate="SW" pin="NC2" pad="6"/>
<connect gate="SW" pin="NO1" pad="1"/>
<connect gate="SW" pin="NO2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIGIKEY" value="563-1105-6-ND"/>
</technology>
</technologies>
</device>
<device name="-GF1260159" package="GF1260159">
<connects>
<connect gate="SW" pin="C1" pad="C1"/>
<connect gate="SW" pin="C2" pad="C2"/>
<connect gate="SW" pin="NC1" pad="NC1"/>
<connect gate="SW" pin="NC2" pad="NC2"/>
<connect gate="SW" pin="NO1" pad="NO1"/>
<connect gate="SW" pin="NO2" pad="NO2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_NAV_TSW" prefix="SW">
<description>C&amp;K TSWB-3N-CB111-LFS
central select with jog and 4 directions (dial &amp; direction ring)&lt;br&gt;
&lt;br&gt;
white - TSWB-3N-CB111 LFS&lt;br&gt;
black - TSWB-3N-CB222 LFS&lt;br&gt;</description>
<gates>
<gate name="SW" symbol="TSWB3NCB111LFS"/>
</gates>
<devices>
<device name="" package="TSWB3NCB111LFS">
<connects>
<connect gate="SW" pin="A" pad="A"/>
<connect gate="SW" pin="B" pad="B"/>
<connect gate="SW" pin="COM_A" pad="COMA"/>
<connect gate="SW" pin="COM_B" pad="COMB"/>
<connect gate="SW" pin="S1" pad="S1"/>
<connect gate="SW" pin="S2" pad="S2"/>
<connect gate="SW" pin="S3" pad="S3"/>
<connect gate="SW" pin="S4" pad="S4"/>
<connect gate="SW" pin="S5" pad="S5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW-1UM" prefix="S">
<description>Switch</description>
<gates>
<gate name="SW" symbol="SWITCH-1UM"/>
</gates>
<devices>
<device name="-A1LD" package="DB3C">
<connects>
<connect gate="SW" pin="C1" pad="C"/>
<connect gate="SW" pin="NC1" pad="NC"/>
<connect gate="SW" pin="NO1" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MSS13PLP" package="MSS13PLP">
<connects>
<connect gate="SW" pin="C1" pad="C"/>
<connect gate="SW" pin="NC1" pad="NC"/>
<connect gate="SW" pin="NO1" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SKS06LP" package="SKS06LP">
<connects>
<connect gate="SW" pin="C1" pad="C"/>
<connect gate="SW" pin="NC1" pad="NC"/>
<connect gate="SW" pin="NO1" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MSS13LSP" package="MSS13LSP">
<connects>
<connect gate="SW" pin="C1" pad="C"/>
<connect gate="SW" pin="NC1" pad="NC"/>
<connect gate="SW" pin="NO1" pad="NO"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_1NC" prefix="SW">
<description>Switch NC</description>
<gates>
<gate name="SW" symbol="SWITCH-1NC"/>
</gates>
<devices>
<device name="-PMC-1001THY" package="PMC-1001THY">
<connects>
<connect gate="SW" pin="C1" pad="1"/>
<connect gate="SW" pin="NC1" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_1NO" prefix="SW">
<description>Switch NO</description>
<gates>
<gate name="SW" symbol="SWITCH-1NO"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
